   3 Server: NetWare 3.11 server
                                                                    v1.08


NetWare* 3.11 Server Driver Installation Notes for the Intel
EtherExpress(TM) PRO/100+ PCI Adapter
============================================================

Location of driver: \NWSERVER\311LAN\100BLAN.EXE 

Overview
--------
NetWare 3.11 requires an ODI 3.2 Assembly Specification driver.  This
driver is in a self-extracting archive named 100BLAN.EXE contained on
the \NWSERVER\311LAN\ directory of the Configuration and Drivers disk.
To unpack the archive copy it to a blank floppy disk and type E100BLAN
on the command line. The archive contains the following files:

     E100B.LAN (3.2 spec server driver)
     E100B.LDI (installation file)
     NW311.TXT (installation instructions)

Refer to NW311.TXT contained in the archive to install the driver.



*  Third-party trademarks are the property of their respective owners.
